{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[17,2,17,3],[18,2,18,3],[20,2,20,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9911006506403321"]
[null,null,"Titolo",null,"AASHTO guide specifications for LRFD seismic bridge design"]
[null,null,"Pubbl/distr/stampa",null,": American Association of State Highway and Transportation Officials (AASHTO)"]
[null,null,"Soggetti",null,"Bridges - Design and construction - Specifications - United States"]
[{"$nulls":4},"Bridges - Earthquake effects"]
[{"$nulls":4},"Earthquake resistant design"]
[{"$nulls":4},"Structural analysis (Engineering)"]
[{"$nulls":4},"Earthquake hazard analysis"]
[{"$nulls":4},"Strains and stresses"]
[{"$nulls":4},"Elastic analysis (Engineering)"]
[{"$nulls":4},"Load factor design"]
[{"$nulls":4},"Soil-structure interaction"]
[{"$nulls":4},"Soil mechanics"]
[{"$nulls":4},"Shear strength of soils"]
[{"$nulls":4},"Shear flow"]
[{"$nulls":4},"Seismic waves - Damping"]
[{"$nulls":4},"Energy dissipation"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,"Nota di contenuto",null,"section 1. Introduction -- section 2. Definitions and notation -- section 3. General requirements -- section 4. Analysis and design requirements -- section 5. Analytical models and procedures -- section 6. Foundation and abutment design -- section 7. Structural steel components -- section 8. Reinforced concrete components -- References -- Appendix A: Foundation-rocking analysis -- Appendix B: Design flowcharts."]
[null,null,null,"Sommario/riassunto","Covers seismic design for typical bridge types and applies to non-critical and non-essential bridges. Approved as an alternate to the seismic provisions in the AASHTO LRFD Bridge Design Specifications. Differs from the current procedures in the LRFD Specifications in the "]
[{"$nulls":4},"use of displacement-based design procedures, instead of the traditional force-based R-Factor method. Includes detailed guidance and commentary on earthquake-resisting elements and systems, global design strategies, demand modeling, capacity calculation, and liquefaction effects. Capacity design procedures underpin the Guide Specifications' methodology; includes prescriptive detailing for plastic hinging regions and design requirements for capacity protection of those elements that should not experience damage.--"]