{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[4,2,4,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[12,2,12,3],[13,2,13,3],[17,2,17,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9911019841503321"]
[null,null,"Titolo",null,"RFID and the internet of things / / edited by Herve Chabanne, Pascal Urien, Jean-Ferdinand Susini"]
[null,null,"Pubbl/distr/stampa",null,"London, : ISTE"]
[{"$nulls":4},"Hoboken, N.J., : Wiley, 2011"]
[null,null,"ISBN",null,"1-118-61429-1"]
[{"$nulls":4},"1-299-31506-2"]
[{"$nulls":4},"1-118-61443-7"]
[null,null,"Descrizione fisica",null,"1 online resource (299 p.)"]
[null,null,"Collana",null,"ISTE"]
[null,null,"Disciplina",null,"384.6"]
[null,null,"Soggetti",null,"Radio frequency identification systems"]
[{"$nulls":4},"Embedded Internet devices"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"pt. 1. Physics of RFID -- pt. 2. RFID applications -- pt. 3. Cryptography of RFID -- pt. 4. EPCglobal -- pt. 5. Middleware."]
[null,null,null,"Sommario/riassunto","RFID (Radio Frequency Identification) technology allows for automatic identification of information contained in a tag by scanning and interrogation using radio frequency (RF) waves.An RFID tag contains an antenna and a microchip that allows it to transmit and receive. This technology is a possible alternative to the use of barcodes, which are frequently inadequate in the face of rapid growth in the scale and complexity of just-in-time inventory requirements, regional and international trade, and emerging new methods of trade based on it. Use of RFID tags will likely eventually become as w"]