{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[19,2,19,3],[20,2,20,3],[24,2,24,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9911019992603321"]
[null,null,"Titolo",null,"Inkjet technology for digital fabrication / / edited by Ian M. Hutchings and Graham D. Martin"]
[null,null,"Pubbl/distr/stampa",null,"Chichester, West Sussex, U.K., : Wiley, 2013"]
[null,null,"ISBN",null,"9781118452943"]
[{"$nulls":4},"1118452941"]
[{"$nulls":4},"9781118452936"]
[{"$nulls":4},"1118452933"]
[{"$nulls":4},"9781299187283"]
[{"$nulls":4},"1299187285"]
[{"$nulls":4},"9781118452929"]
[{"$nulls":4},"1118452925"]
[null,null,"Edizione",null,"[1st edition]"]
[null,null,"Descrizione fisica",null,"1 online resource (562 p.)"]
[null,null,"Disciplina",null,"620.1/06"]
[null,null,"Soggetti",null,"Microfluidics"]
[{"$nulls":4},"Microfabrication"]
[{"$nulls":4},"Ink-jet printing"]
[{"$nulls":4},"Three-dimensional printing"]
[{"$nulls":4},"Coating processes"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Includes index."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"Introduction to inkjet printing for manufacturing -- Fundamentals of inkjet technology -- Dynamics of piezoelectric print-heads -- Fluids for inkjet printing -- When the drop hits the substrate -- Manufacturing of Micro-Electro-Mechanical (MEMS) -- Conductive tracks and passive electronics -- Printed circuit board fabrication -- Active electronics -- Flat-panel Organic Light-Emitting Diode (OLED) displays : a case study -- Radiofrequency Identification (RFID) manufacturing : a case study -- Biopolymers and cells -- Tissue engineering : a case study -- Three-dimensional digital fabrication -- Current inkjet technology and future directions."]
[null,null,null,"Sommario/riassunto","Whilst inkjet technology is well-established on home and small office desktops and is now having increasing impact in commercial printing, it can also be used to deposit materials other than ink as individual droplets at a microscopic scale. This allows metals, ceramics, polymers "]
[{"$nulls":4},"and biological materials (including living cells) to be patterned on to substrates under precise digital control. This approach offers huge potential advantages for manufacturing, since inkjet methods can be used to generate structures and functions which cannot be attained in other ways.  Beginning with an ov"]