{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[16,2,16,3],[17,2,17,3],[20,2,20,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9911020226803321"]
[null,null,"Autore",null,"Munjiza Ante"]
[null,null,"Titolo",null,"The combined finite-discrete element method / / Ante Munjiza"]
[null,null,"Pubbl/distr/stampa",null,"Hoboken, NJ, : Wiley, c2004"]
[null,null,"ISBN",null,"9786610274857"]
[{"$nulls":4},"9781280274855"]
[{"$nulls":4},"1280274859"]
[{"$nulls":4},"9780470020173"]
[{"$nulls":4},"0470020172"]
[{"$nulls":4},"9780470020180"]
[{"$nulls":4},"0470020180"]
[{"$nulls":4},"9780470020172"]
[null,null,"Descrizione fisica",null,"1 online resource (x, 333 pages)"]
[null,null,"Disciplina",null,"620.1/123/015118"]
[null,null,"Soggetti",null,"Deformations (Mechanics) - Mathematical models"]
[{"$nulls":4},"Finite element method"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references (pages 319-330) and index."]
[null,null,"Nota di contenuto",null,"Processing of contact interaction in the combined finite discrete element method -- Contact detection -- Deformability of discrete elements -- Temporal discretisation -- Sensitivity to initial conditions in combined finite-discrete element simulations -- Transition from continua to discontinua -- Fluid coupling in the combined finite-discrete element method -- Computational aspects of combined finite-discrete element simulations -- Implementation of some of the core combined finite-discrete element algorithms."]
[null,null,null,"Sommario/riassunto","The combined finite discrete element method is a relatively new computational tool aimed at problems involving static and / or dynamic behaviour of systems involving a large number of solid deformable bodies. Such problems include fragmentation using explosives (e.g rock blasting), impacts, demolition (collapsing buildings), blast loads, digging and loading processes, and powder technology.The combined finite-discrete element method - a natural extension of both discrete and finite element methods - allows researchers to model problems involving the deformability of either one solid body,"]