{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[14,2,14,3],[15,2,15,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279338103316"]
[null,null,"Titolo",null,"High-voltage switchgear and controlgear . Part 37-082, Standard practice for the measurement of sound pressure levels on alternating current circuit-breakers - Redline / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway : , : IEEE, , 2012"]
[null,null,"ISBN",null,"0-7381-8390-3"]
[null,null,"Edizione",null,"[2012(E)(Revision of IEEE Std C37.082-1982).]"]
[null,null,"Descrizione fisica",null,"1 online resource (44 pages)"]
[null,null,"Collana",null,"IEC/IEEE 62271-37-082"]
[null,null,"Disciplina",null,"621.317"]
[null,null,"Soggetti",null,"Electric switchgear"]
[{"$nulls":4},"Electric controllers - Standards"]
[{"$nulls":4},"High voltages"]
[{"$nulls":4},"Sound pressure"]
[{"$nulls":4},"Electric circuit-breakers"]
[{"$nulls":4},"Electric circuits - Alternating current"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This standard provides methods for the measurement of sound pressure level produced by outdoor alternating current circuit-breakers in a free-field environment. These methods may also be used indoors or in restricted field, provided that precautions are observed in the measurement and interpretation of the results."]