{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279339903316"]
[null,null,"Titolo",null,"IEC/IEEE 62582-2 Edition 1.0 2016-02 : IEC/IEEE International Standard for Nuclear power plants -- Instrumentation and control important to safety -- Electrical equipment condition monitoring methods -- Part 2: Indenter modulus - Amendment 1 / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway, NJ, USA : , : IEEE, , 2016"]
[null,null,"ISBN",null,"1-5044-0792-X"]
[null,null,"Descrizione fisica",null,"1 online resource (14 pages)"]
[null,null,"Disciplina",null,"621.4835"]
[null,null,"Soggetti",null,"Nuclear power plants - Safety measures"]
[{"$nulls":4},"Nuclear reactors - Safety measures"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This International Standard contains methods for condition monitoring of organic and polymeric materials in instrumentation and control systems using the indenter modulus technique in the detail necessary to produce accurate and reproducible measurements. It includes the requirements for the selection of samples, the measurement system and measurement conditions, and the reporting of the measurement results. Standards in the IEC/IEEE 62582-series are measurement standards, primarily for use in the management of ageing in initial qualification and after installation. IEC/IEEE 62582-1 General includes requirements for the application of the IEC/IEEE 62582-series and some elements which are common to all methods. Information on the role of condition monitoring in qualification of equipment important to safety is found in IEEE Std 323. This standard is intended for application to non-energised equipment."]