{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279861703316"]
[null,null,"Titolo",null,"ANSI/IEEE Std 1101-1987 / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : IEEE, , 1988"]
[null,null,"ISBN",null,"0-7381-4142-9"]
[null,null,"Descrizione fisica",null,"1 online resource (55 pages)"]
[null,null,"Disciplina",null,"004.16"]
[null,null,"Soggetti",null,"Microcomputers"]
[{"$nulls":4},"Electronic digital computers"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","The standard covers three areas: the basic dimensions of subracks, this range of modular subracks conforming to IEC 297-3-1984, for mounting in equipment according to IEC 297-1-1986, and ANSI/EIA RS-310, together with the basic dimensions of a compatible range of plug-in units, printed boards, and backplanes; the dimensions of plug-in units and connectors, this standard gives the dimensions of associated plug-in units and connectors standardized by IEC 603-2-1980, together with applicable detail dimensions of the subrack; and the environmental requirements of subracks, this standard states environmental requirements of subracks and their associated plug-in units. The purpose of the standard is the specification of dimensions that will ensure the mechanical interchangeability and environmental requirements of subracks and of plug-in units."]