{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[10,2,10,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280059403316"]
[null,null,"Titolo",null,"IEC/IEEE 60255-118-1:2018 IEEE/IEC International Standard - Measuring relays and protection equipment . Part 118-1, Synchrophasor for power systems - Measurements / / Power System Relaying and Control of the IEEE Power and Energy Society"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 2018"]
[null,null,"ISBN",null,"1-5044-5361-1"]
[null,null,"Descrizione fisica",null,"1 online resource (78 pages)"]
[null,null,"Collana",null,"IEC/IEEE ; ; 60255-118-1"]
[null,null,"Disciplina",null,"621.3815322"]
[null,null,"Soggetti",null,"Phase converters"]
[{"$nulls":4},"Electric relays"]
[{"$nulls":4},"Electric measurements"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This document provides continuation and further development of previous synchrophasor standards, notably the IEEE C37.118 series. It defines synchrophasor, frequency, and rate of change of frequency (ROCOF) measurements as used in this technology. These definitions are in agreement with most research on and analysis of dynamic electric power system measurements, but may differ from those given in other contexts. Function and performance requirements are given for synchrophasor measurements. Tests, evaluation criteria, and error limits are provided to determine compliance with the requirements."]