{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[7,2,7,3],[7,4,7,5],[8,2,8,3],[8,4,8,5],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[15,2,15,3],[16,2,16,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280400803316"]
[null,null,"Titolo",null,"2013 IEEE/RSJ International Conference on Intelligent Robots and Systems"]
[null,null,"Pubbl/distr/stampa",null,"IEEE"]
[null,null,"ISBN",null,"1-4673-6358-8"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,"2.","Record Nr.",null,"UNISA996279883103316"]
[null,null,"Titolo",null,"ANSI/IEEE C57.12.00-1980 : American National Standard General Requirements for Liquid-Immersed Distribution, Power, and Regulating Transformers / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : IEEE, , 1980"]
[null,null,"ISBN",null,"1-5044-0514-5"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Disciplina",null,"621.314"]
[null,null,"Soggetti",null,"Electric transformers"]
[{"$nulls":4},"Electric current regulators"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This standard is intended as a basis for the establishment of performance, limited electrical and mechanical interchangeability, and safety requirements of equipment described; and for assistance in the proper selection of such equipment. This standard describes electrical, mechanical, and safety requirements of liquid-immersed distribution and power transformers, and autotransformers and regulating transformers; single and polyphase, with voltage 601 V or higher in the highest voltage winding. This standard applies to all liquid-immersed distribution, power, and regulating transformers except as indicated below: (1) Instrument transformers. (2) Step-voltage and induction voltage regulators. (3) Arc furnace transformers. (4) Rectifier transformers. (5) Specialty transformers. (6) Grounding transformers. (7) Mobile transformers. (8) Mine transformers. When this standard is used on a mandatory basis, the words shall and must indicates mandatory requirements; and the words should and may."]