{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280416303316"]
[null,null,"Titolo",null,"IEEE Std 802.11d-2001 : IEEE Standard for Information Technology - Telecommunications and Information Exchange Between Systems - Local and Metropolitan Area Networks - Specific Requirement. Part 11: Wireless LAN Medium Access Control (MAC) and Physical La / / Institute of Electrical and Electronics Engineers (IEEE)"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : Institute of Electrical and Electronics Engineers (IEEE), , 2001"]
[null,null,"Descrizione fisica",null,"1 online resource (viii, 26 pages) : illustrations"]
[null,null,"Disciplina",null,"004.68"]
[null,null,"Soggetti",null,"Local area networks (Computer networks) - Standards"]
[{"$nulls":4},"Wireless LANs - Standards"]
[{"$nulls":4},"C (Computer program language)"]
[{"$nulls":4},"Computer interfaces - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","\"This amendment specifies the extensions to IEEE Std 802.11 for Wireless Local Area Networks providing specifications for conformant operation beyond the original six regulatory domains of that standard. These extensions provide a mechanism for an IEEE Std 802.11 access point to deliver the required radio transmitter parameters to an IEEE Std 802.11 mobile station, which allows that station to configure its radio to operate within the applicable regulations of a geographic or political subdivision. This mechanism is applicable to all IEEE Std 802.11 PHY types. A secondary benefit of the mechanism described in this amendment is the ability for an IEEE Std 802.11 mobile station to roam between regulatory domains.\"."]