{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280459503316"]
[null,null,"Titolo",null,"IEEE Standard Specifications for Surge Protectors Used in Low-Voltage Data, Communications,and Signaling Circuits / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York, N.Y. : , : IEEE, , 2009"]
[null,null,"ISBN",null,"0-7381-6090-3"]
[null,null,"Edizione",null,"[(Revision of IEEE Std C62.64-1997).]"]
[null,null,"Descrizione fisica",null,"1 online resource (80 pages) : illustrations"]
[null,null,"Collana",null,"IEEE Std ; ; C62.64-2009"]
[null,null,"Disciplina",null,"621.3"]
[null,null,"Soggetti",null,"Low voltage integrated circuits"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,null,"Sommario/riassunto","Surge protectors for application on multiconductor and coaxial, balanced or unbalanced, data, communications, and signaling circuits with voltages less than or equal to 1000 V rms or 1200 V dc are covered. These surge protectors are multiple-component series or parallel combinations of one or more nonlinear elements and zero or more linear elements. The tables of typical performance values provide a means of comparison among various surge protectors. They also provide a common engineering language beneficial to the user and manufacturer of surge protectors used in low-voltage data, communications, and signaling circuits."]