{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[10,2,10,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280748203316"]
[null,null,"Titolo",null,"IEEE Std 1455-1999 : IEEE Standard for Message Sets for Vehicle/Roadside Communications / / Vehicular Technology Society Rail Transit Vehicle Interface Standards Committee, Institute of Electrical and Electronics Engineers, IEEE-SA Standards Board"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 1999"]
[null,null,"ISBN",null,"0-7381-1770-6"]
[null,null,"Descrizione fisica",null,"1 online resource (vi, 130 pages) : illustrations"]
[null,null,"Collana",null,"IEEE Std ; ; 1455-1999"]
[null,null,"Disciplina",null,"388.312"]
[null,null,"Soggetti",null,"Highway communications"]
[{"$nulls":4},"Highway communications - Data processing - Standards"]
[{"$nulls":4},"Intelligent transportation systems"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Those characteristics of a dedicated short-range communications (DSRC) system thatare independent of the Physical and Data Link Layers (ISO model Layers 1 and 2) are specified.The required and optional features of the roadside equipment (RSE) and the onboard equipment(OBE) are specified. In addition, the Applications Layer (ISO model Layer 7) services and protocols,the RSE resource manager, the corresponding OBE command interpreter, and the application-spe-cific messages are all specified. Standard supports and guidelines are provided for implementingsecure DSRC systems."]