{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280749303316"]
[null,null,"Titolo",null,"IEEE Std 1390-1995 : IEEE Standard for Utility Telemetry Service Architecture for Switched Telephone Network / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway, New Jersey : , : IEEE, , 1996"]
[null,null,"ISBN",null,"0-7381-0572-4"]
[null,null,"Descrizione fisica",null,"1 online resource (32 pages)"]
[null,null,"Disciplina",null,"621.37"]
[null,null,"Soggetti",null,"Electric meters - Standards"]
[{"$nulls":4},"Telephone systems - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Withdrawn Standard. Withdrawn Date: Feb 06, 2006. This standard describes a utility telemetry service architecture operated over the telephone network. The architecture described is a basic transport architecture capable of supporting many different applications. The text is described in terms of a utility meter reading application, but any enhanced service provider (ESP) communication can be transported. Telemetry calls may be initiated by either the utility/service provider (outbound) or the telemetry interface unit (TIU)/CPE (inbound) on the end user's premise."]