{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280991503316"]
[null,null,"Titolo",null,"ISO/IEC/IEEE Standard for Information. technology . Part 4, Mixed-mode communication protocols and Transducer Electronic Data Sheet (TEDS) : Smart transducer interface for sensors and actuators / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York, N.Y. : , : IEEE, , 2010"]
[null,null,"ISBN",null,"0-7381-6275-2"]
[null,null,"Descrizione fisica",null,"1 online resource (448 pages) : illustrations"]
[null,null,"Collana",null,"ISO/IEC/IEEE ; ; 21451-4:2010(E)"]
[null,null,"Disciplina",null,"681.2"]
[null,null,"Soggetti",null,"Sensor networks"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,null,"Sommario/riassunto","This standard defines the protocol and interface that allows analog transducers to communicate digital information with an IEEE 1451 object. It also defines the format of the Transducer TEDS. The Transducer TEDS is based on the IEEE 1451.2™ TEDS. The standard does not specify the transducer design, signal conditioning, or the specific use of the TEDS."]