{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996575086803316"]
[null,null,"Titolo",null,"1685-2022 : IEEE Standard for IP-XACT, Standard Structure for Packaging, Integrating, and Reusing IP within Tool Flows / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , [2023]"]
[null,null,"ISBN",null,"1-5044-9448-2"]
[null,null,"Descrizione fisica",null,"1 online resource (750 pages)"]
[null,null,"Disciplina",null,"620.0042"]
[null,null,"Soggetti",null,"Engineering design"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Conformance checks for eXtensible Markup Language (XML) data designed to describe electronic systems are formulated by this standard. The meta-data forms that are standardized include components, systems, bus interfaces and connections, abstractions of those buses, and details of the components including address maps, register and field descriptions, and file set descriptions for use in automating design, verification, documentation, and use flows for electronic systems. A set of XML schemas of the form described by the World Wide Web Consortium (W3C(R)) and a set of semantic consistency rules (SCRs) are included. A generator interface that is portable across tool environments is provided. The specified combination of methodology-independent meta-data and the tool-independent mechanism for accessing that data provides for portability of design data, design methodologies, and environment implementations."]