{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996575170303316"]
[null,null,"Titolo",null,"1635-2022 - IEEE/ASHRAE Guide for the Ventilation and Thermal Management of Batteries for Stationary Applications / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York, USA : , : IEEE, , 2022"]
[null,null,"ISBN",null,"1-5044-9140-8"]
[null,null,"Descrizione fisica",null,"1 online resource (140 pages)"]
[null,null,"Disciplina",null,"697.92"]
[null,null,"Soggetti",null,"Ventilation"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Vented lead-acid (VLA), valve-regulated lead-acid (VRLA), nickel-cadmium (Ni-Cd - both fully vented and partially-recombinant types), and Li-ion stationary battery installations are discussed in this guide, written to serve as a bridge between the electrical designer and the heating, ventilation, and air-conditioning (HVAC) designer. Ventilation of stationary battery installations is critical to improving battery life while reducing the hazards associated with hydrogen production (hydrogen production is not a concern with Li-ion under normal operating conditions [it is under thermal runaway conditions]). This guide describes battery operating modes and the hazards associated with each. It provides the HVAC designer with the information to provide a cost effective ventilation solution."]