{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[4,2,4,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[10,2,10,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996575626503316"]
[null,null,"Titolo",null,"\"C57.12.34-2022 - IEEE Standard Requirements for Pad-Mounted, Compartmental-Type, Self-Cooled, Three-Phase Distribution Transformers, 10 MVA and Smaller; High-Voltage, 34.5 kV Nominal System Voltage and Below; Low-Voltage, 15 kV Nominal System Voltage and Below\" / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 2022"]
[{"$nulls":4},"©2022"]
[null,null,"ISBN",null,"9781504491747"]
[{"$nulls":4},"1504491742"]
[null,null,"Descrizione fisica",null,"1 online resource (56 pages)"]
[null,null,"Disciplina",null,"621.319"]
[null,null,"Soggetti",null,"Electric power distribution"]
[{"$nulls":4},"Electric transformers"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Certain electrical, dimensional, and mechanical characteristics are set forth, as well as certain safety features of three-phase, 60 Hz, liquid-immersed, self-cooled, pad-mounted, compartmental-type distribution transformers. These transformers are rated 10 MVA and smaller, with the high-voltage limit of 34.5 kV nominal system voltage and below, and with low-voltage limit of 15 kV nominal system voltage and below. This standard covers the connector, bushing, and terminal arrangements for radial or loop-feed systems. This standard does not cover the electrical and mechanical requirements of any accessory devices that may be supplied with the transformer."]